**Overview**

Designed specifically to meet the needs of the highly competitive retail ATM market, the Genmega G1900 combines the features you expect with a flexible platform that allows you to customize it to fit your location and traffic volume.

**Advantages**

* Strong security points, including reinforced edges along the vault's door and a flashing security LED
* Versatile enough to support popular dispense models such as De La Rue SDD and the Puloon LCDM 1000.
* Highly customizable to fit the needs of your business
* Include custom advertisements on the 7-inch LCD screen

**Features**

* Optional high-brightness toper sign that accepts custom inserts
* Highly visible LED sign to attract customers
* 8 customizable ad screens
* ADA voice guidance, lighted action indicators, and accessible keypad layout

**Specifications**

* Display: 7-inch diagonal 32-bit color, backlit TFT LCD panel, and 800 x 480 WVGA
* Printer: 56mm thermal receipt printer
* PIN Entry Device: 16-key alphanumeric keypad, VISA/PCI and Interact Certified, Triple-DES (TDES) compliant EPP
* Cash Dispenser: 800 note fixed cassette (TCDU), 1,000 note removable cassette (SCDU), 1,700 note removable cassette (MCDU), 2 x 1,700 note multi-cassette (MCDU), and optional support for De La Rue SDD and Puloon LCDM 1,000
* CPU: Samsung S3C2440AL-40 RISC 32-bit CPU, 64 MB RAM/Windows CE 5.0 OS, and electronic journal > 40,000 transactions
* Communication: 56,000 bps dial-up modem and TCPIP Ethernet connection – onboard SSL
* Card Reader: Dual-head swipe card reader and optional EMV – DIP
* Security: UL291 business hours vault, door seam reinforcement, and dial or electronic lock
* Power Requirements: 110/220 VAC, 50/60 Hz, 145 watts
* Environmental Conditions: 32 – 104°F (0 – 49° C), 15 – 85% humidity
* Height: 56.36 inches
* Width 15.75 inches
* Depth: 22.29 inches
* Weight: 206 pounds