**Overview**

The Genmega G2500 comes with the standard features you expect from an ATM machine, but a variety of optional upgrades make it highly-customizable to fit your business needs. From the high-resolution LCD display to the receipt printer, you can truly make this ATM your own. The G2500 is specifically designed for retail and off-premise locations.

**Advantages**

* Upgrade the receipt printer to add 3-inch graphics for custom branding or coupons
* The 8-inch high-resolution wide screen LCD can be upgraded to a 10.2-inch touch screen.
* The machine supports cash dispensers from other equipment suppliers, making it even more flexible.

**Features**

* Optional LED topper sign that can accept custom inserts
* Highly visible LED sign that attracts customers
* ADA complaint with voice guidance, lighted transaction guidance, and an accessible keypad layout

**Specifications**

* Display: 8-inch diagonal 32-bit color backlit TFT LCD panel with 800 x 480 resolution
* Printer: 56mm (2-inch) with optional 80mm (3-inch)
* Pin Entry Device: 16-key alphanumeric keypad, PCI/Interact Certified, and Triple DES (TDES) complaint EPP
* Communication: 56kb internal model and TCP/IP Ethernet – SSL
* CPU: Samsung 32-bit CPU with 64 MB RAM/Windows CE 5.0
* Card Reader: DIP type with optional EMV
* Security: UL291 business hours vault and dial or electronic lock
* Cash Dispenser: 800 note fixed cassette (TCDU), 1,000 note removable cassette (SCDU), 1,700 note removable cassette (MCDU), and 2 x 1,700 note removable cassette (MCDU)
* Power Requirements: 110/220 VAC, 50/60 Hz, 145 watts
* Environmental Conditions: 45 – 95°F (5 – 35°C), 15 – 85% humidity
* Height: 56.3 inches
* Width: 15.8 inches
* Depth: 22.3 inches
* Weight 206 pounds