**Overview**

If you are looking for a through-the-wall ATM machine, look no further than the GT3000 from Genmega. An economic solution for business owners, it is ideal for small and compact areas, kiosks, and anywhere space is minimal.

**Advantages**

* Weather-resistant chassis makes the GT3000 a great option for outdoors
* Compact machine fits in the smallest of spaces
* Rear service panel provides secure loading and management functions
* Uses existing Genmega components so maintenance remains easy

**Features**

* High visibility LED sign to attract customers
* Optional rear service panel
* ADA complaint with voice guidance, lighted transaction guidance, and accessible keypad layout

**Specifications**

* Display: 7-inch diagonal 32-bit color, backlit TFT LCD panel, 800 x 480 resolution, and customizable ad screens
* Printer: 56mm (2-inch standard)
* Pin Entry Device: 16-key alphanumeric keypad, PCI/Interac Certified, and triple-DES (TDES) complaint EPP
* Communication: 56kb internal model and TCP/IP Ethernet – SSL
* CPU: Samsung 32-bit CPU, 64MB RAM/Windows CE 5.0
* Card Reader: DIP type card reader with optional EMV
* Security: UL291 business hours vault and dial or electronic lock
* Cash Dispenser: 800 note fixed cassette (TCDU), 1,700 note rear-load removable cassette)
* Power Requirements: 110/220 VAC, 50/60 Hz, 145 watts
* Environmental Conditions: 45 – 95°F (5 – 35°C), 15 – 85% humidity
* Height: 33.8 inches
* Width: 15 inches
* Depth: 30 inches
* Weight: 182 pounds